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CAD FILE REQUIREMENTS

For each land development project, a cad file is required to be submitted to Gainesville Regional Utilities at each iteration for the project.  Each CAD file must be georeferenced in the following horizontal and vertical coordinate system:
· Horizontal -Florida State Plane Coordinates, AND 83 Zone North US Survey feet 
· Vertical - NAVD 88 datum with elevations given in US survey feet. 

Cad files shall be placed in the CAD File folder found in Project Dox.  

Please be aware of the specifications listed below. Please have the CAD file formatted as requested. 
Please provide an AutoCAD file ROTATED TO NORTH. 
Required layers:
· Survey/parcel boundary (4 property corners are required)
· Proposed edge of pavement
· Proposed sidewalk/concrete, face of curb, back of curb, etc…
· Proposed Building footprints
· Proposed utilities easements
· Proposed electrical features (from GRU mark-up)
· Proposed Public and Private Sewer Mains and Laterals
· Proposed Water Main Service Lines, Blow-offs and Valves, and other fitting
· Proposed Reclaimed Water Main, Service Lines, Valves and other fittings
· Proposed Force Mains, including valves and ARVs
· Proposed Gas features (from GRU mark-up)
· Other proposed above and below ground utilities.
· Proposed Retention basins


NOTE: Please remove x-references and bind referenced drawing(s) 
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